1- می توان با استفاده از ip netns exec h1 این کار را کرد.

۲-

۳-ip netns exec netns1 ip addr add 172.17.42.99/16 dev eth0

4-Virtual Ethernet interfaces are an interesting construct; they always come in pairs, and they are connected like a tube—whatever comes in one veth interface will come out the other peer veth interface. As a result, you can use veth interfaces to connect a network namespace to the outside world via the “default” or “global” namespace where physical interfaces exist.

5-ip link add veth0 type veth peer name veth1

6-ip link set veth1 netns blue

7-لیست دیوایس های شبکه و مشخصاتشان چاپ می شود